gwire can be plugged into nce command station

when plugged in will act as a pro cab

when on wireless - uses selectable wireless channels

sending full DCC commands via wireless - no RB02

for live track systems - power thru rail, no dcc

loco has wireless receiver, decoder, and booster

for dead rail, wireless receiver, decoder, and booster and battery

decider from CVP air wire / qsi

stubby 1/4 wave roughly has 30% less range then full 1/2 wave antenna

to get firmware version, turn off radio system, hit red btn on throttle

current version is 1.5 has much better range,