**Cab bus Device Current draw FAQ**

Procab Throttle 85mA - back light flicker = low voltage

Cab04 30mA

Cab05 35mA

Cab06 50mA

RB02 60mA

RPT1 35mA

AIU 24mA at idle / 90mA at full load

UTP 30 mA

UTP Cat5 30 mA

Mini Panel 60 mA

USB interface 30mA

Available Cab Bus capacity supplied from command station

CS02 -/ PH-Pro / Power Pro cab bus 1 amp

Powercab - subtracted from total power (2A)