
Blue / C is always the lighting (+) common  
White is (-) for front headlight  
Yellow is (-) for rear headlight  
  
Orange is Motor (+)  
Gray is Motor (-)  
Red is track power, right rail  
Black is track power, left rail    
  
CV33 F0F    default value is 1    output 1 / white  / pin 6  
CV34 F0R        default value is 2      output 2 / yellow / pin 2  
CV35 F1        default value is 4      output 3 / green  / pin 3  
CV36 F2        default value is 8      output 4 / violet    
  
CV120 EFX for F0F output 1 / white  / pin 6        default value is 1  directional active in Forward  
CV121 EFX for F0R output 2 / yellow / pin 2        default value is 2  directional active in Reverse    
CV122 EFX for F1 output 3 / green / pin 3          default value is 0 - standard on / off    
CV123 EFX for F2 output 4 / violet                default value is 0 - standard on / off    
  
​