To reset MTH to the address to factory default 3.

Set the engine on the main, enter up loco #55, to into

program on main. program loco 55, CV 55 with a value of 55.

exit out and call up loco 3,

perform start up by press F3 to start loco.

If you want to re enable long addressing

at this point, go back into programming for loco 3,

at CV29 enter a value of 38.

F7 to cycle thru 9 volume levels

F8 for smoke